**Title: Manuscript instructions (16 points, bold)**

Authour(s):（12 points）

*Affiliation(s): (9 points, 斜体)*

Keywords:（9 points）

The text: (10.5 points)

* ワープロソフトは、Wordでお願いします。
* ページ設定は、＜文字数と行数＞　「行数だけを指定する」をチェックし、

　　　　　　　　　　行数：３６　に指定してください。

　　　　　　　　　＜余白＞　上：３５mm　下：３０mm　左：２０mm　右：２０mm

　（ただし、本文が長かったり、図が入ったりした場合は、一枚でおさまるよう＜余白＞

部分以外を調整いただいて結構です。）

* フォントは　Times　か　Times　New　Roman　でお願いします。
* Title　から　Keywordまではセンタリングしてください。
* 本文は両端揃えで、行頭を半角英数５文字分あけ、1段落でまとめて下さい。
* 図を載せられる場合は、全て含めてA4一枚におさまるよう、貼り付けてください。
* グラフ、図は白黒印刷で分かるよう作成してください。
* ファイル名の最初は第一著者のイニシャルで始めてください。たとえば，第一著者名がHaruki Murakamiであった場合は，ファイル名を”HM\_abstract.doc”としてください。
* 次ページの例をご参照下さい。

以上よろしくお願い致します。

**The effects of noise exposure on temporary damage in hair cells**

**of Mongolian gerbils evaluated by the cochlear microphonics**

Keizo Fukushima1 , Kohta I. Kobayasi2 , Andrea M. Simmons2,3, James Simmons2,3 ,

and Hiroshi Riquimaroux1,2

*1Sensory & Cognitive Neural System Laboratory, Graduate School of Life and Medical Science, Doshisha University*

*2Neurosensing and Bionavigation Research Center, Doshisha University, Kyotanabe, Kyoto 610-0321, Japan*

*3Department of Neuroscience, Brown University 185 Meeting St Box G-LN Providence, RI 02912*

**Keywords:** Cochlear nonlinearity, Outer hair cells, Awake preparation, Round window, Hearing sensitivity, SPL dependency

High intensity noise exposure can cause temporary or permanent hearing loss. In this study, we evaluated the temporary damage in hair cells by the cochlear microphonics (CM) in Mongolian gerbils (*Meriones unguiculatus*), which communicate with each other with vocalizations and have an audible range similar to humans. Adult gerbils received surgical implantation of a silver wire electrode on the round window of their cochlea through the middle ear to record CM. After the surgery, they were exposed to broadband noise (0.5 to 45 kHz) at 90 dB SPL for 5 minutes. CMs were recorded for tone bursts of 1 to 45 kHz. The following results were obtained. First, we observed the largest CM reduction just after the noise exposure. Second, decrements in CM amplitude depended on frequency sensitivity. In other words, low sensitivity frequency range above 22 kHz produced large reduction in CM amplitude. Third, decrease in CM amplitude was greater for lower stimulus intensities. Fourth, for testing frequencies, which produced large CM decrements, it took a longer period to recover back to pre-noise exposure amplitude levels. These findings indicate that reduction in CM amplitude appeared to be related to the cochlear nonlinearity generated by the outer hair cells.

Fig. 1 CM amplitude shift levels in dB compared with pre and post noise exposures. **A**: 80 dB SPL sound stimuli. **B**: 40 dB SPL sound stimuli. Black bar: noise bandwidth. For both **A** and **B**, slight temporary damages were observed. For 80 dB SPL (**A**), CM decreased equally at all frequency. On the other hand, with 40dB SPL (**B**), remarkable CM shift was observed in the high frequency range (22 kHz to 45 kHz).

